**Specifications for Aqueous Sulfolane**

Specific gravity @ 20/20 **◦C** - 1.26 - 1.27

Purity (dry basis), wt% - 99.5 (min)

Water, wt% - 2.6 - 3.0

Ash, wt% - 0.10 ( max )

Thermal Stability test, PPM SO2 - 30 ( max )

2 Sulfolane, wt% - 0.2 ( max )

Isopropylsulfolanyl ether, wt% - 0.3 ( max )

**DISTILLATION:**

% Volume recovered at 282 **◦C**  - 05 ( max )

% Volume recovered at 288 **◦C** - 95 ( max )